# Point Results

Use the Point Results tab to view all the vertex points found in the calibration plate.

All fields in the Point Results tab are read only. The uncalibrated point results are reported in the selected space coordinates of the calibration image, while the raw calibrated point results are reported in the raw calibrated coordinate space.

Select any point result to highlight the point on the Current.CalibrationImage buffer (and on the Current.UndistortedCalibrationImage buffer is warping is in effect).