# GigE

Use the GigE tab to view basic information about the connected GigE Vision camera and modify various GigE Vision properties.

The Camera Information section of the tab presents basic information regarding the camera and adapter you are using. Use the Feature Access area to examine and modify the XML-defined properties for the GigE Vision camera you are using.

- Enter the XML node name in the Feature field.
- Clicking Read will read the value of the node and update the Value field.
- Clicking Write will attempt to write whatever value is in the Value field to the node.
- Clicking Execute will attempt to execute the command feature specified in the Feature field.

QuickBuild will display a dialog box for any errors that occur, such an invalid entry for the Feature or Value fields. Refer to the documentation for the GigE Vision camera you are using for a list of supported XML nodes.