# VisionView Web Panel Display Specifications

Specification | Description
Micro SD Card | Micro SD Slot × 1
LCD | 9” WSVGA TFT-LCD
Resolution | 1024 x 600
Touchscreen | Resistive / Capacitive
USB | USB 2.0 × 2
Ethernet | Integrated 10/100/1000 Mbps Ethernet
Power Input | Multi-Voltage +8 ~ +35 V DC
Operating Temperature | 0°C to +60°C
Storage | -30°C to +80°C
Humidity | 0% ~ 90% relative humidity, non-condensing
IP Rating | IP65 (front panel)
Shock | Yes
Vibration | Yes