# Mount VisionView Web Panel on Table Top Stand

1. Insert two M4 hex screws to the top mounting holes of the VisionView Web panel without fully tightening them.

2. Slide the VisionView Web panel on the table top stand so that the screws catch onto the notches in the stand.

3. Tighten the screws completely.

Optionally, you can use the three screw holes on the bottom of the stand to attach the table top stand to a horizontal surface.