# Mount VisionView Web Panel to FastMount Bracket

You can use the FastMount bracket to attach the VisionView Web Panel to any surface that has a suitable opening to accommodate the device. For the required size of the cutout, see VisionView Web Panel Dimensions.

1. Attach the gasket to the back of the VisionView Web panel.

2. Position the FastMount bracket to the back of the VisionView Web panel. Align the mounting holes of the bracket with the screw holes of the panel, then insert and tighten the four hex screws.

3. Rotate the VisionView Web panel and insert it into the cutout until the gasket is flush with the mounting surface.

4. Insert the four fasteners into the respective holes without tightening them.

5. Slide on the end cap of each fastener.

6. Hand-tighten all four fasteners until the VisionView Web panel is securely fixed.