To transfer Images from In-Sight Vision Suite:

1. Launch In-Sight Vision Suite and connect to your device with the Spreadsheet Connect button.

2. Make sure that the Filmstrip contains images.

3. Drag-and-drop the Toolchain Contains a group of tools and the sequence of execution for each tool. function from the In-Sight Toolbox to the spreadsheet.

   The Toolchain property sheet pops up.

4. Click Login on the property sheet.

   The Authenticating... window pops up.

5. Enter your email address and click Continue.

   The User field in the property sheet now shows your username.

6. Select your project In OneVision, a project is a collection of images and vision tools that performs different tasks, such as inspection, measurement, or identification. in OneVision from the Project dropdown and click Open, or create a new project by clicking the New button.

7. Log in to the OneVision project on the login screen.

   OneVision opens. The Spreadsheet cell is now connected to the Input Image The set of images used to train and test your vision application. tool in OneVision.

8. Switch back to In-Sight Vision Suite.

9. Click OK to close the property sheet.

10. Collect images from the Filmstrip to transfer to OneVision:

    1. Enable the Collect Images checkbox on the Toolchain function.

    2. Double-click on an image in the Filmstrip to select it.

       Tip: All Filmstrip controls that change the displayed frame can add images to the collection.

    3. Click on the Clear Images button to remove all images from the current collection.

    The Num Images field of the Toolchain function indicates the number of images you selected.

11. Open the Toolchain tool property sheet.

12. Click Upload Images.

    The Uploading Images pop-up appears. Click Cancel to terminate image transfer. When the pop-up disappears, the images are available in OneVision.

13. Verify that the images are available in OneVision by opening the Input Image tool and checking the images.