After training, adjust Process step parameters to accurately inspect the image dataset.

1. Set the appropriate process parameters. Process parameters vary based on the train mode and model selected.

   Processing Parameters

   Processing Parameter | Description
   Minimum Blob Area | Filters out results with an area smaller than this value.
   Threshold | Values below the threshold are the view background. Values above are the foreground.
   Simple Region | Check the box to simplify and remove inner holes in the region.

2. After you set the parameters, click Process All.

3. Review the inspection results for your image data set. For more information, see Metrics and Statistics.