You can use images from In-Sight Vision Suite in your OneVision project In OneVision, a project is a collection of images and vision tools that performs different tasks, such as inspection, measurement, or identification.. Using the Toolchain Contains a group of tools and the sequence of execution for each tool. function in spreadsheet, you can collect, tag, and transfer images from the Filmstrip or from live image acquisition. The image collection method is similar to collecting images with the ViDiEL tools.

You can access the image collection from a file explorer if needed. The images are stored locally on the vision sensor and they are deleted after you upload them to OneVision.

Before you start, ensure that the Filmstrip contains images.

To transfer images from In-Sight Vision Suite:

1. Add a Toolchain function to the spreadsheet.

2. In the Property Sheet of the Toolchain function:

   1. Log in to OneVision.

   2. Select a project in the Project dropdown.

   3. Check the Collect Images checkbox.

   4. Click OK to close the Property Sheet and apply your changes.

3. Load images from the Filmstrip into the Toolchain function.

   - To add images one by one, double-click the desired images in the Filmstrip.

   - Click the Play button in the Filmstrip controls to load all of the images in the Filmstrip.

   - The Num Images field of the Toolchain function indicates the number of images in the collection.

   - Once you have loaded the images, uncheck the checkbox in the Collect Images cell of the function.

4. Review the images in the collection.

   1. Open the Property Sheet of the Toolchain function and go to the Images tab.

   2. To help you manage your image collection, add tags to your images. The tags are uploaded to OneVision together with the images.

   3. Delete duplicate or unneeded images from the collection.

5. To upload the images to OneVision, click Upload Images in the Property Sheet of the Toolchain function.

Note: If you collect images but do not upload them, the images can stay in the storage of the vision sensor, taking up storage space.

To verify that the images are available in OneVision, open the Input Image The set of images used to train and test your vision application. tool in OneVision and check the images.