# Create an Advanced Recipe

You can locate and align a part by creating a recipe with two features. For example, one feature could be a corner and the other feature could be a fiducial. This recipe applies in these situations:

- The camera shuttles between two positions with a stationary part.
- The part shuttles between two positions with a stationary camera.

- The part and camera are stationary; the part has two features in the field of view, so that you can train them individually.

1. To open the New Recipe dialog box, click .

1. Type the Name and Description of the recipe.
2. Click to close the dialog box.
3. Click to display the Advanced Recipe Settings.

4. Choose Shuttling camera or Shuttling part based on the item you are moving. Of choose No shuttling if you have one part with two features in the field of view.

1. Use the normal procedure to define the feature including the Image Setup and Pattern definition.

1. Once you have defined Feature 1, click Feature 2 and define that feature.

2. Click at the bottom right to finish the recipe definition..