### SLMP

As opposed to TCP connection, the SLMP connection supports loading a Recipe. This is performed as follows:

- Set Master In-Sight offline by setting the “Set Offline” bit in the control block to 1

- Wait for the “Online” Bit in the Status Block to be 0

- Set the “RecipeID” field in the Vision Input Data Block to the desired recipe’s ID

- Start the load process of the recipe with setting the “Load Job” bit in the Control Block

- Wait for the “Job Load Completed” bit in the status block

- Set Master In-Sight online by by setting the “Set Offline” bit in the control block to 0

- Wait for the “Online” Bit in the Status Block to be 1