# Image Size and Dimensions

The figures in the table below, for example the maximum number of images per stream, are experimentally tested and the values vary depending on your hardware configuration. The more memory (not GPU RAM) and hard disk capacity you have, the more and larger images you can handle. As the number and the size of images get larger, the training and processing time for all images increases as well.

Tool | Tool Architecture | Minimum Size | Maximum Size (Channel Parameter Set to 1 to 4) | Maximum Images per Stream | Maximum Trained Features per Image | Maximum Discrete Labeled Features | Maximum Number of Classes | Maximum Number of Defects per Image
Blue Locate | N/A | N/A | Images up to 32MP (up to 16k in height or width) are supported. Images up to 32k pixels wide (in one dimension, dependent upon GPU resources). Images over 32k are not supported. | 25000 | 1000 | 256 | N/A | N/A
Blue Read
Green Classify | Focused | N/A | 25000 | N/A | N/A | 200 | N/A
High Detail
Red Analyze | Focused | N/A | 1000 | N/A | N/A | N/A | 1000
High Detail | 96 x 96 (pixels)