Intel Core i7 or higher.

- The Blue Locate tool is sensitive to clock speed rates, particularly with complex model A specific spatial arrangement of a set of features (Blue Locate and Blue Read tools only.) During a post-processing step, the Blue Locate and Blue Read tools can fit all of the features detected in an image to the models defined for the tool. The overall pose and identity of the model is then returned. matching applications.

- If a single core performs multiple tasks, processing time can increase. Therefore, use a sufficient amount of resources or allocate only one task to a single core.