You can use images from In-Sight Vision Suite in your OneVision project. Using the OneVision function in spreadsheet, you can collect, tag, and transfer images from the Filmstrip or from live image acquisition. The image collection method is similar to collecting images with the Edge AI tools.

You can access the image collection from a file explorer if needed. The images are stored locally on the vision system and they are deleted after you upload them to OneVision.

Before you start, ensure that the Filmstrip contains images.

To transfer images from In-Sight Vision Suite:

1. Add a OneVision function to the spreadsheet.

2. In the Property Sheet of the OneVision function:

   1. Log in to OneVision.

   2. Select a project in the Project dropdown.

   3. Check the Collect Images checkbox.

   4. Click OK to close the Property Sheet and apply your changes.

3. Load images from the Filmstrip into the OneVision function.

   - To add images one by one, double-click the desired images in the Filmstrip.

   - Click the Play button in the Filmstrip controls to load all of the images in the Filmstrip.

   - The Num Images field of the OneVision function indicates the number of images in the collection.

   - Once you have loaded the images, uncheck the checkbox in the Collect Images cell of the function.

4. Review the images in the collection.

   1. Open the Property Sheet of the OneVision function and go to the Images tab.

   2. To help you manage your image collection, add tags to your images. The tags are uploaded to OneVision together with the images.

   3. Delete duplicate or unneeded images from the collection.

5. To upload the images to OneVision, click Upload Images in the Property Sheet of the OneVision function.

Note: If you collect images but do not upload them, the images can stay in the storage of the vision system, taking up storage space.

To verify that the images are available in OneVision, open the Input Image tool in OneVision and check the images.