# Acquiring Images Manually

In the case of manual acquisition, the project typically has:

- A Task that has its trigger mode set to "Manual" (Figure 1), with a Task that has a Camera Device in it (with the acquired image bound to a tag).
- A Page with a Button User Controls, which is bound to Tasks.Task.Run and runs the Task when pressed, and, optionally, a VisionPro Display Vision control bound to the tag of the acquired image.

When the user presses the Button, the camera device acquires an image (and displays it in the VisionPro Display control, if exists).

Figure 1: A Task configured to be triggered manually.