# Cameras

Cognex Designer supports several types of cameras and frame grabbers, and up to four cameras (either physical or simulated) may be connected. This can be any combination of Cognex Industrial Cameras (CIC), as well as the Cognex Displacement Sensor (DS) 3D sensors.

Note: For more information regarding which specific cameras and frame grabbers are supported in Cognex Designer, please consult the cameras.html file, which is included with the VisionPro software, in the Doc directory of the VisionPro installation.