# SLMP Status Word Signal Table

The SLMP Status Word signal table/block organizes the word length signals sent FROM the vision system to the PLC. The size of the Status Word block can vary, depending on the size of the inspection results section.

Byte | 16 Bit Word
--- | ---
0 | Current Job ID
1 | Error ID
2 | Acquisition ID 0
3 | Inspected Image ID 0
4 | Inspection Result Code 0
5 | Acquisition ID 1
6 | Inspected Image ID 1
7 | Inspection Result Code 1
8 | Acquisition ID 2
9 | Inspected Image ID 2
10 | Inspection Result Code 2
11 | Acquisition ID 3
12 | Inspected Image ID 3
13 | Inspection Result Code 3
14-1920 | Inspection Results