# Status

The Status WebPage elements are used to insert HMI elements that graphically display the status of the inspection or another WebPage element. This WebPage element category contains the following components.

Element | Description
Multi Status | Inserts a control for graphically displaying the status of an Integer value of another WebPage Controls element, or an Integer Tag in the project, that is bound to the element's Value property. This element can be used to represent a binary representation of an Integer value, a history of results or the states of the Precision I/O lines in a project. The MultiStatus element has three additional Event handler script points: On Value Change On Mouse Down On Mouse Up The MultiStatus control's numbering is zero-based, and you can define the first bit to be displayed by setting the Start Bit (default is 0). The control determines the order of the displayed bits by first applying the Start Bit property, and then the value of the Reverse Order property. The following illustration indicates how the control's settings can be used to display different bit values:
Progress Bar | Inserts a control to display the progress of a process, by selecting a user-defined Minimum and Maximum (starting and end points) properties, and the Value property to monitor. These properties can either be bound to tags or hard-coded. The progress of the value is determined based on the ratio of the Value property to the Minimum and Maximum properties (starting and end points). Note: The Progress Bar element does not have any Event handler script points.
Status | Inserts a control to graphically display the status of an integer value in the project, by binding the Value property to either a Tag or another value in the project. In addition, text, colors and icons can be added to help define the status being displayed. When monitoring the Value: > 0 = Positive 0 = Zero < 0 = Negative The Status element has three additional Event handler script points: On Value Change On Mouse Down On Mouse Up