View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How can I see errors in the device log using scripting?

Use the Throw() command to report the occurrence of an anomalous situation (exception) and the error will appear in the device log when the device is not connected to Setup Tool. You can access the error log by clicking, in the Setup Tool's menu bar, System, and then Show Device Log.

While the device is connected to Setup Tool, the exception appears below the the script on the scrip pane.

Note: DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370,DM280, DM470,DM580, DM503,DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500