View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# DotCode Properties

Specifying the number of data rows and columns

Specifying the minimum and maximum number of data rows and columns can improve the ability of the reader to reliably decode symbols.

Polarity setting

You can set what the device defines as a module (dot) in relation to its background. The Dark on Light setting implies that the device scans for and decodes dark dots on a light background, while Light on Dark is the opposite (light dots on a dark background).

The default Either setting scans for both kind of modules on their respective background, but this may lead to a slightly slower decoding.

Note: DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370,DM280, DM470,DM503,DM7500,DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500