View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Multicode

Allow Partial Results

Enable Allow Partial Results to allow the reader to return a successful read result when the image contains fewer codes than the Number of Codes specifies.

Allow Identical 1D Symbols

Enable Allow Identical 1D Symbols to allow the reader to return multiple results in an image even if the reader detects more than one symbol (in the same image) with the same length, symbology, and data string.

Allow Identical 1D Symbols applies only to two or more identical 1D symbols that appear in one single image. The Allow identical 1D Symbol control has no effect on images taken one after the other (regardless of mode) even if the same identical symbol is found.

Sorting Priority

The list for Sorting Priority allows you to determine how the reader reports multiple results.

- Use the Up and Down buttons to move any option to a higher or lower priority.

- Use the Reverse button to reverse the order within a selected option.

- Be aware that the Position options (Top to Bottom or Left to Right) refer to the center of the symbols.

- Use Image Order for the Burst or Continuous trigger modes, where symbols that are decoded in earlier images are reported before symbols decoded in later images.

Note: DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM503,MX-1000,MX-1500