View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do I view multicode results?

To enable multicode results, you must increase the Number of Codes parameter from the default value of 1 on the Multicode tab in the Symbology Settings pane.

If your reader detects and decodes multiple symbols in the same image, each symbol appears outlined in green and the Read Result History grid displays a single line displaying all the decoded data concatenated on one line. The results are separated and followed by the ASCII characters for CR (<0x0d>) and LF (<0x0a>). To view the separate results for each symbol, click the "+" sign next to the concatenated results.

As you click on an individual result, the Image Viewer will highlight the corresponding symbol.

Note: default,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM503