# Charging Station Specifications

Specification | Charging Station
--- | ---
Weight | 380 g
Operating Temperature | 0ºC — +40ºC (+32ºF — +104ºF)
Storage Temperature | -40ºC — +60ºC (-40ºF — +140ºF)
Charging Temperature | 0ºC — +35ºC (+32ºF — +95ºF)
Maximum Humidity | 95% (non-condensing)
Environmental | IP40
Power Supply Requirements | 24 V, 24 W maximum LPS or NEC Class 2 power supply 0.5A (inductive) and 1A (non-inductive)

Note: The operating and charging temperature may be lower depending on the installed mobile phone.