View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What does Transfer All Images do?

Check Transfer All Images to view all the burst images associated with each trigger.

When checked, all images acquired in burst mode will be accessible from the Result History pane, regardless of whether any image contains a decoded result or not.

This option is only available if you select Burst for the trigger type in the Advanced tab of Optimize Image pane.

Note: If the Output Delay is shorter than the reader needs to acquire an image and decode for any results, Setup Tool may not receive result images from the reader.

Note: default,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM380, DM503