View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Why is my DataMan returning multiple results in response to a single trigger?

This can happen when the hardware trigger input line is being used because the signal on the line is oscillating around its final value, and the reader interprets the oscillations as separate trigger signals. Increasing the Debounce Delay in the System Settings pane's Inputs tab can cause the reader to interpret all the oscillations as a single trigger signal.

Note: default,DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM380, DM503