# INPUT.ACTION

Sets or gets the state for the specified line action.

Note: The input actions "Train Code," "Optimize Brightness," "Set Match String," and "Read Configuration Code" are carried out only after the next trigger.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
line |  | [0-3] | Input line number
action |  | [0-11] | 0: Train Code 1: Optimize Brightness 2: Set Match String 3: Optimize Focus 4: Read Configuration Code 5: Trigger Off 6: Encoder 7: Allow Buffered No-Read Images 8: Clear Outputs 9: Tune (DM300 only) 10: Encoder direction 11: Trigger on
state |  | [ON|OFF] | ON: execute action when line is triggered OFF: no action

## Platforms

Fixed-mount readers

## Notes

Version: 4.0.0