# WIFI.BAND

802.11 frequency band of the network. Associations to the Wi-Fi network locked to the specific band.

Note: If you set WIFI.BAND to any value other than 0, attempts to set WIFI.SCAN-CHANNELS to anything but an empty string fail with error code 104. Attempting to set WIFI.BAND to a non-zero value while the value of WIFI.SCAN-CHANNELS is not an empty string results in a failure with error code 104.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
band | int | [0-2] | 0: Any band 1: 2.4 GHz band 2: 5 GHz band

## Platforms

DM8700 Wi-Fi reader

## Notes

Version: 6.2.6