View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the Image Size (Region of Interest) setting used for?

You can use this feature to specify the exact region of the image the reader will use to locate and decode a symbol. This can be helpful if two Data Matrix codes are in close proximity to each other and you need to ensure you only read the code along the target aiming line. Reducing the region of interest does not necessarily reduce the decoding time or increase the image transfer rate.

You can set a different region of interest for each setup, if your device supports multiple setups.

Note: DM7500,DM8600,DM8700,MX-1000,MX-1500