View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Where can I change power management settings for the MX-1000/MX-1500?

You can use the Inactivity Timeouts settings to configure timeouts related to power. Unless Disable Power Off Mode is ticked, the device will power down automatically after the time elapses set under Enter power off mode after (s).

You can either drag the slider or enter a value into the text box.

Note: The device automatically switches on from Power Off Mode if any of the three buttons (Left Trigger, Right Trigger, Grip Button) are pushed.

Note: MX-1000,MX-1500