View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How can I have the Primary reader report all code results from each reader in the Multi-Reader Sync group?

In Multi-Reader Sync mode, the Primary reader can be configured to report its own code results and all code results from all of the Secondary readers. In order to do this, on the Symbology Settings pane's Multicode tab, you must configure the Number of Codes setting for the Primary reader. This must be set to the total number of codes you would like to see returned from the Multi-Reader Sync group.

For example, if you have a Primary reader and a Secondary reader each reading a single code, then the Number of Codes setting for the Primary reader would be 2. If the Secondary reader was reading 3 codes and the Primary reader was reading 1, then Number of Codes on the Primary reader would be set to 4. The Number of Codes setting on the Primary reader can be varied from 1 to total number of codes read by all readers in a single Multi-Reader Sync group.

Note that if a Secondary reader is reading multiple codes, you must also configure the Secondary reader's Multicode settings so that it will read and return multiple code results to the Primary reader.

Note: DM060,DM070,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM380, DM503