View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What do I use the Report FTP Transfer tab for?

The Report FTP Transfer tab allows you to set up code quality results to be sent via FTP in form of an HTML report. You must tick the checkbox Enable Code Quality Report Transfer to allow the device to send results through FTP and identify the server you want to send data to by providing the server address, username, password, and type of the server.

Idle Timeout is the amount of time that a port is held open with no outgoing traffic. Once the reader opens a connection to an FTP server, the reader keeps that connection open as long as traffic occurs. If no traffic occurs for the set Idle Timeout period, the connection is closed. This can be useful if an FTP transfer only happens seldom and the network overhead for keeping the connection open is not desired. You need to check Enable Idle Timeout first to be able to set the idle timeout.

Settings under File Name govern FTP report file name generation. There are options available to set up:

- Custom File Name generation: select this option if you want to provide the file name yourself. You can specify the name under File Name. The File Name field accepts not only file names, but also path names. Use forward slashes as delimiter. For example, /images/image. Append settings allow you to set the numbering rules for file name generation: Max Append Value sets the maximum number the file names’ numbering goes, Max Append Start Value sets where the file name numbering starts.

- Script Generated File Name: after enabling this option, click on the blue option name to navigate immediately to Scripting > FTP Transfer, where the sample script for file name generation is already provided.

- Server Generated File Name: provide the server address here after selecting this option to generate report file names based on a server. Some FTP servers support this functionality to uniquely name incoming files before saving them to disk.

Note: DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM380, DM503,MX-1000,MX-1500