# CAMERA.GAIN

Gets or sets the sensitivity of the image sensor. A higher number means higher sensitivity, which also increases image noise.

Note: The gain has no effect if the camera runs with automatic exposure.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
gain | float | [1.00-15.00] | DM50, DM60, DM70
[1.00-125.59] | DM80, DM280
[1.00-32.00] | DM282
[1.00-31.76] | DM300, DM360
[1.00-251.18] | DM370, DM470
[1.00-13.88] | DM503

## Platforms

DM50, DM60, DM70, DM80, DM280, DM300, DM360, DM370, DM470, DM503

## Notes

Version: 5.5.0