# COM.USB-HID-IGNORE-CAPS-LOCK

When the HID Ignore Caps Lock command is ON, the reader detects the Caps Lock state of the host computer and any alphabetical character is converted to the opposite case, so the exact read string encoded into the code (Datamatrix, QR code, etc.) appears on the screen of the computer.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
type | bool | [ON|OFF] | enable/disable

## Platforms

DM80-USB, DM280, DM8700 base station USB, DM8700 USB

## Notes

Version: 6.2.2