# CAMERA.EXPOSURE-US

Camera Parameters where exposure is in microseconds. The argument 'exposure' and 'gain' has no effect if 'auto' is ON and 'target' has no effect at all.

Note: This command is deprecated for the listed platforms. It is recommended to use the CAMERA.EXPOSURE command instead.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
auto | bool | [ON|OFF] | ON: Automatic OFF: Manual
target | int | [0-255] | target pixel value
exposure | int | [43-200000] | DM80, DM280
[30-200000] | DM282
[15-200000] | DM370, DM470
[27-400000] | DM580
[43-200000] | DM8700
gain | float | [1-125.59] | DM80, DM280
[1-32.00] | DM282
[1-251.18] | DM370, DM470
[1-24.00] | DM580
[1-251.18] | DM8700

## Platforms

DM80, DM280, DM370, DM470, DM580, DM8700

## Notes

Version: 5.5.0