View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# I'm having trouble reading codes on my parts. What should I do?

- Make sure that you press and hold the trigger. If you release the trigger before the read is complete, the reader abandons its read attempt.

- Verify that the reader is within the working distance specified for the code size and type, as listed in the Scan Map document.

- Make sure that you have the code centered within the image area of the reader and that the code is centered within the green aiming light before you pull the trigger.

- Click on Light Settings on the Advanced tab of Optimize Image pane (UltraLight Settings for DM7500 and DM8600,DM8700), then adjust the lighting settings.

- Click on Symbology Settings and make sure that the symbology type you are using is enabled.

Note: DMAE50,DM7500,DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500