# Data Formatting Tokens

## General Tokens

Token | Description
--- | ---
<BRDC> | Total No-Reads
<CANG> | Code Orientation
<CCTR> | Code Center
<CNTR> | Contrast
<CPOS> | Code Position
<CRLF> | CR/LF
<DATA> | Full String
<DSUB> | Sub-string. For example <DSUB(1-2)>.
<FVDC> | Failed Validation
<GRDC> | Total Reads
<IALT> | Image acquisition local time
<IAUT> | Image acquisition UTC time
<ICNT> | Buffered Allowed No Reads
<IGEN> | Result Source
<IRCLT> | Subresult creation local time
<IRCUT> | Subresult creation UTC time
<ISTR> | Input String
<ITFL> | Filter Time
<LTIM> | Current local time
<MOSI> | Module Size
<MTRG> | Missed Triggers
<PCMR> | PCM Data
<PVDC> | Passed Validation
<RDSI> | Used Read Setup
<SMID> | Symbology Identifier
<SMSI> | Symbol Size
<SPAC> | SP
<SYMB> | Symbology
<TABS> | TAB
<TCLT> | Trigger creation local time
<TCUT> | Trigger creation UTC time
<TELT> | Trigger execution local time
<TEUT> | Trigger execution UTC time
<TIDX> | Trigger Index
<TMDC> | Decode Time
<TMTR> | Trigger Time
<TTRG> | Total Triggers
<UTIM> | Current UTC time
<UUEC> | Unused Error Correction

## Validation Tokens

Token | Description
--- | ---
<AI00> | Serial Shipping Container Code (SSCC)
<AI01> | Global Trade Item Number
<AI02> | GTIN of Contained Trade Items
<AI10> | Batch or Lot Number
<AI11> | Production Date
<AI12> | Due Date for Amount on Payment Slip
<AI13> | Packaging Date
<AI15> | Best Before Date
<AI16> | Sell By Date
<AI17> | Expiration Date
<AI20> | Product Variant Number
<AI21> | Serial Number
<AI240> | Additional Product Identification Assigned by the Manufacturer
<AI241> | Customer Part Number
<AI242> | Made-to-Order Variation Number
<AI243> | Packaging Component Number
<AI250> | Secondary Serial Number
<AI251> | Reference to Source Entity
<AI253> | Global Document Type Identifier (GDTI)
<AI254> | GLN Extension Component
<AI255> | Global Coupon Number (GCN)
<AI30> | Variable Count of Items
<AI310x> | Net weight (kilograms)
<AI311x> | Length or first dimension
<AI312x> | Width, diameter, or second dimension
<AI313x> | Depth, thickness, height, or third dimension
<AI314x> | Area (sq meters)
<AI315x> | Net Volume (liters)
<AI316x> | Net Volume (cubic meters)
<AI320x> | Net Weight (pounds)
<AI321x> | Length or first dimension (inches)
<AI322x> | Length or first dimension (feet)
<AI323x> | Length or first dimension (yards)
<AI324x> | Width, diameter, or second dimension (inches)
<AI325x> | Width, diameter, or second dimension (feet)
<AI326x> | Width, diameter, or second dimension (yards)
<AI327x> | Depth, thickness, height, or third dimension (inches)
<AI328x> | Depth, thickness, height, or third dimension (feet)
<AI329x> | Depth, thickness, height, or third dimension (yards)
<AI330x> | Logistic weight (kilograms)
<AI331x> | Length or first dimension (meters)
<AI332x> | Width, diameter, or second dimension (meters)
<AI333x> | Depth, thickness, height, or third dimension (meters)
<AI334x> | Area (sq meters)
<AI335x> | Logistic volume (liters)
<AI336x> | Logistic volume (cubic meters)
<AI337x> | Kilograms Per Square Metre
<AI340x> | Logistic weight (pounds)
<AI341x> | Length or first dimension (inches)
<AI342x> | Length or first dimension (feet)
<AI343x> | Length or first dimension (yards)
<AI344x> | Width, diameter, or second dimension (inches)
<AI345x> | Width, diameter, or second dimension (feet)
<AI346x> | Width, diameter, or second dimension (yards)
<AI347x> | Depth, thickness, height, or third dimension (inches)
<AI348x> | Depth, thickness, height, or third dimension (feet)
<AI349x> | Depth, thickness, height, or third dimension (yards)
<AI350x> | Area (sq inches)
<AI351x> | Area (sq feet)
<AI352x> | Area (sq yards)"
<AI353x> | Area (sq inches)
<AI354x> | Area (sq feet)
<AI355x> | Area (sq yards)
<AI356x> | Net weight (troy ounces)
<AI357x> | Net weight or volume (ounces)
<AI360x> | Net volume (quarts)
<AI361x> | Net volume (gallons us)
<AI362x> | Logistic volume (quarts)
<AI363x> | Logistic volume (gallons us)
<AI364x> | Net Volume (cubic inches)
<AI365x> | Net Volume (cubic feet)
<AI366x> | Net Volume (cubic yards)
<AI367x> | Logistic volume (cubic inches)
<AI368x> | Logistic volume (cubic feet)
<AI369x> | Logistic volume (cubic yards)
<AI37> | Count of Trade Items Contained in a Logistic Unit
<AI390x> | Amount Payable - Single Monetary Area
<AI391x> | Amount Payable and ISO Currency Code
<AI392x> | Amount Payable for a Variable Measure Trade Item - Single Monetary Area
<AI393x> | Amount Payable for a Variable Measure Trade Item and ISO Currency Code
<AI400> | Customer's Purchase Order Number
<AI401> | Global Identification Number for Consignment (GINC)
<AI402> | Global Shipment Identification Number (GSIN)
<AI403> | Routing Code
<AI410> | Ship to - Deliver to Global Location Number
<AI411> | Bill to - Invoice to Global Location Number
<AI412> | Purchased from Global Location Number
<AI413> | Ship for - Deliver for - Forward to Global Location Number
<AI414> | Identification of a Physical Location - Global Location Number
<AI415> | Global Location Number of the Invoicing Party
<AI420> | Ship to - Deliver to Postal Code within a Single Postal Authority
<AI421> | Ship to - Deliver to Postal Code with Three-Digit ISO Country Code
<AI422> | Country of Origin of a Trade Item
<AI423> | Country of Initial Processing
<AI424> | Country of Processing
<AI425> | Country of Disassembly
<AI426> | Country Covering Full Process Chain
<AI427> | Country Subdivision of Origin Code for a Trade Item
<AI7001> | Stock Number (NSN)
<AI7002> | UN/ECE Meat Carcasses and Cuts Classification
<AI7003> | Expiration Date and Time
<AI7004> | Active Potency
<AI7005> | Catch Area
<AI7006> | First Freeze Date
<AI7007> | Harvest Date
<AI7008> | Species for Fishery Purposes
<AI7009> | Fishing Gear Type
<AI7010> | Production Method
<AI703x> | Number of Processor with Three-Digit ISO Country Code
<AI710> | National Healthcare Reimbursement Number (Germany)
<AI711> | National Healthcare Reimbursement Number (France)
<AI712> | National Healthcare Reimbursement Number (Spain)
<AI713> | National Healthcare Reimbursement Number (Brazil)
<AI8001> | Roll Products - Width, Length, Core Diameter, Direction, Splices
<AI8002> | Cellular Mobile Telephone Identifier
<AI8003> | Global Returnable Asset Identifier (GRAI)
<AI8004> | Global Individual Asset Identifier (GIAI)
<AI8005> | Price per Unit of Measure
<AI8006> | Identification of the Components of a Trade Item
<AI8007> | International Bank Account Number (IBAN)
<AI8008> | Date and Time of Production
<AI8010> | Component / Part Identifier
<AI8011> | Component / Part Identifier Serial Number
<AI8017> | Global Service Relation Numbers (GSRN) - Provider
<AI8018> | Global Service Relation Numbers (GSRN) - Recipient
<AI8019> | Service Relation Instance Number (SRIN)
<AI8020> | Payment Slip Reference Number
<AI8100> | GS1-128 Coupon Extended Bar Code
<AI8101> | GS1-128 Coupon Extended Bar Code
<AI8102> | GS1-128 Coupon Extended Bar Code
<AI8110> | Coupon Code Identification for Use in North America
<AI8200> | Extended Packaging URL
<AI90> | Information Mutually Agreed Between Trading Partners
<AI91> | Company Internal Information
<AI92> | Company Internal Information
<AI93> | Company Internal Information
<AI94> | Company Internal Information
<AI95> | Company Internal Information
<AI96> | Company Internal Information
<AI97> | Company Internal Information
<AI98> | Company Internal Information
<AI99> | Company Internal Information
<VEID> | Enterprise Identifier
<VPNU> | Part Number
<VSNU> | Serial Number
<VUID> | Unique Item Identifier

## Code Quality Tokens

### Data Matrix - ISO/IEC 15415

Token | Description
--- | ---
<ANG1> | Axial Non-uniformity 15415 Grade
<ANM1> | Axial Non-uniformity 15415 Metric
<CCG1> | Cell Contrast 15415 Grade
<CCM1> | Cell Contrast 15415 Metric
<EXR0> | Extreme Reflectance Grade
<FPD1> | Fixed Pattern Damage Grade 15415
<GNG1> | Grid Non-uniformity 15415 Grade
<GNM1> | Grid Non-uniformity 15415 Metric
<MOD1> | Modulation 15415
<PGG1> | Print Growth Grade 15415
<PGM1> | Print Growth Metric 15415
<UEG1> | Unused Error Correction 15415 Grade
<UEM1> | Unused Error Correction 15415 Metric

### Data Matrix - ISO/IEC TR 29158 (AIM DPM)

Token | Description
--- | ---
<ANG0> | Axial Non-uniformity AIM-DPM Grade
<ANM0> | Axial Non-uniformity AIM-DPM Metric
<CCG0> | Cell Contrast AIM-DPM Grade
<CCM0> | Cell Contrast AIM-DPM Metric
<FPD0> | Fixed Pattern Damage Grade
<GNG0> | Grid Non-uniformity AIM-DPM Grade
<GNM0> | Grid Non-uniformity AIM-DPM Metric
<MOD0> | Modulation AIM-DPM
<MRG0> | Minimum Reflectance AIM-DPM Grade
<MRM0> | Minimum Reflectance AIM-DPM Metric
<UEG0> | Unused Error Correction AIM-DPM Grade
<UEM0> | Unused Error Correction AIM-DPM Metric

### Data Matrix - Semi T10

Token | Description
--- | ---
<CCM0> | Symbol Contrast
<UEM0> | Unused Error Correction
<CDEFG> | Cell Defects Semi-T10 Metric
<DMCHG> | Data Matrix Cell Height Semi-T10 Metric
<DMCWG> | Data Matrix Cell Width Semi-T10 Metric
<FPDFV> | Finder Pattern Semi-T10 Metric
<HMGV> | Horizontal Mark Growth Semi-T10 Metric
<HZMMV> | Horizontal Mark Misplacement Semi-T10 Metric
<SNRV> | Signal to Noise Ratio Semi-T10 Metric
<VMGV> | Vertical Mark Growth Semi-T10 Metric
<VTMMV> | Vertical Mark Misplacement Semi-T10 Metric

### QR - ISO/IEC 15415

Token | Description
--- | ---
<ANG5> | Axial Non-uniformity QR Grade
<ANM5> | Axial Non-uniformity QR Metric
<CCG5> | Cell Contrast Grade
<CCM5> | Cell Contrast Raw
<EXR5> | Extreme Reflectance QR Grade 15415
<FPD5> | Fixed Pattern Damage QR Grade 15415
<GNG5> | Grid Non-uniformity QR Grade 15415
<GNM5> | Grid Non-uniformity QR Metric 15415
<MOD5> | Modulation QR Grade 15415
<PGG5> | Print Growth QR Grade
<PGM5> | Print Growth QR Metric
<UEG5> | Unused Error Correction QR Grade
<UEM5> | Unused Error Correction QR Metric

### QR - ISO/IEC TR 29158 (AIM DPM)

Token | Description
--- | ---
<ANG7> | Axial Non-Uniformity QR Grade
<ANM7> | Axial Non-Uniformity QR Metric
<CCG7> | Cell Contrast QR Grade
<CCM7> | Cell Contrast QR Metric
<FPD7> | Fixed Pattern Damage QR Grade
<GNG7> | Grid Non-uniformity QR Grade
<GNM7> | Grid Non-uniformity QR Metric
<MOD7> | Cell Modulation QR Grade
<MRG7> | Minimum Reflectance QR Grade
<MRM7> | Minimum Reflectance QR Metric
<PGG7> | Print Growth QR Grade
<PGM7> | Print Growth QR Metric
<UEG7> | Unused Error Correction QR Grade
<UEM7> | Unused Error Correction QR Metric

### 1D Readability (Cognex)

Token | Description
--- | ---
<CCG4> | Symbol Contrast 1D Grade
<CCM4> | Symbol Contrast 1D Metric
<ECG4> | Edge Contrast Min 1D Grade
<ECM4> | Edge Contrast Min 1D Metric
<MRG4> | Reflect Min 1D Grade
<MRM4> | Reflect Min 1D Metric
<MSG4> | Multi Scan Integrity 1D Grade
<MSM4> | Multi Scan Integrity 1D Metric
<PGG4> | Print Growth 1D Grade
<PGM4> | Print Growth 1D Barcode Metric
<SSG4> | Single Scan Integrity 1D Grade

### ISO/IEC 15416

Token | Description
--- | ---
<CCG8> | Symbol Contrast 1D Barcode Grade (ISO 15416)
<CCM8> | Symbol Contrast 1D Barcode Metric (ISO 15416)
<DCG8> | Decodability Grade (ISO 15416)
<DCV8> | Decodability Metric (ISO 15416)
<ECG8> | Edge Contrast Minimum Grade (ISO15416)
<ECM8> | Edge Contrast Minimum Metric (ISO15416)
<EDG8> | Edge Determination Grade (ISO 15416)
<EDV8> | Edge Determination Metric (ISO 15416)
<DEG8> | Defects Grade (ISO 15416)
<DEV8> | Defects Metric (ISO 15416)
<MOD2> | Modulation Metric (ISO 15416)
<MOD8> | Modulation Grade (ISO 15416)
<MRG8> | Minimum Reflectance Grade (ISO 15416)
<MRM8> | Minimum Reflectance (ISO15416)
<OVG8> | Overall Grade (ISO 15416)
<OVV8> | Overall Metric (ISO 15416)
<RDC8> | Reference Decode Grade (ISO 15416)
<RDV8> | Reference Decode Metric (ISO15416)

### Dot Code AIM

Token | Description
--- | ---
<ANG6> | Axial Non-uniformity DotCode Grade (* change from AIM Specification thresholds)
<ANM6> | Axial Non-uniformity DotCode Metric
<CCG6> | Cell Contrast DotCode Grade
<CCM6> | Cell Contrast DotCode Metric
<GNG6> | Grid non-uniformity DotCode Grade
<GNM6> | Grid Non-uniformity DotCode Metric
<PGG6> | Print Growth DotCode Grade
<PGM6> | Print Growth DotCode Metric
<UEG6> | Unused Error Correction DotCode Grade
<UEM6> | Unused Error Correction DotCode Metric

### Code Quality

Token | Description
--- | ---
<CBRD> | Consecutive Bad Reads
<PGAV> | Overall Print Growth (Average of H&V)
<PGHZ> | Print Growth Horizontal
<PGVT> | Print Growth Vertical
<PVDC> | Passed Validations
<TDFA> | Dark Field light angle
<TSTA> | Angle Test
<TSTD> | Distortion Test
<TSTP> | Position Test
<CCG2> | Cell Contrast AS9132-LE Grade
<CCM2> | Cell Contrast AS9132-LE Metric
<CUM1> | Contrast Uniformity 15415 Metric
<CUM5> | Contrast Uniformity QR Metric
<DAG2> | Distortion Angle AS9132 Grade
<DAM2> | Distortion Angle AS9132 Metric
<FHG2> | Cell Fill Horizontal AS9132-LE Grade
<FHM2> | Cell Fill Horizontal AS9132-LE Metric
<FVG2> | Cell Fill Vertical AS9132-LE Grade
<FVM2> | Cell Fill Vertical AS9132-LE Metric
<GRD0> | Symbol Grade (AIM-DPM)
<GRD1> | Symbol Grade 15415
<GRD2> | Symbol Grade AS9132-LE
<GRD3> | Symbol Grade AS9132-DP
<PGM0> | Print Growth AIM-DPM Metric
<PSG3> | Position Failure AS9132-DP Grade
<PSM3> | Position Failure AS9132-DP Metric
<RDC0> | Reference Decode AIM-DPM
<RDC1> | Reference Decode 15415
<RMG1> | Reflectance Margin 15415 Grade
<RMG5> | Reflectance Margin QR Grade
<RMM1> | Reflectance Margin 15415 Metric
<RMM5> | Reflectance Margin QR Metric
<SOG3> | Size and Ovality Failure AS9132-DP Grade
<SOM3> | Size and Ovality Failure AS9132-DP Metric