# MIRROR.ANGLE-DIRECT

Sets a new angle pair value and moves the mirror to the given position, without storing it on the path. On Get, returns the last set angle pair value of the mirror. Consider this operation only in non repetitive trigger modes. In case of a single angle motion (e.g. 0, angle_b) the limit expands to 25°. If Mirror2Axis feature key is not present, the a-axis have to be 0, or it gets rejected.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
float | data | [-17° - +17°] | float angle_a
float | data | [-17° - +17°] | float angle_b

## Platforms

DM370, DM470 equipped with High Speed Steerable Mirror

## Notes

Version: 6.1.10