# HPIT.EXPANDED-FOCUS-ENABLED

Enables/Disables the robust focus functionality. When active, the lens scans in equal power steps around a defined power increasing the DoF at a slight decrease of readout time.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
state |  | [ON|OFF] | enable/disable

## Platforms

DM370, DM390 with HPIT, DM470 with HPIT.

## Notes

Version: 6.1.7