# LIGHT.BANKS

LIGHT.BANKS command sets the light banks on the reader. The possible values are ON and OFF for each bank. Example for a SET command: SET LIGHT.BANKS ON OFF OFF if you want to have the Direct illumination on. You can enable both the Direct and Polarized banks at once, but the Diffuse bank can only be enabled exclusively.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
Direct | bool | [ON|OFF] | enable/disable
Polarized | bool | [ON|OFF] | enable/disable
Diffuse | bool | [ON|OFF] | enable/disable

## Platforms

DM80, DM280, DM290, DM8700 DX

## Notes

Version: 6.2.0