# PTP.SLAVE-ONLY

This parameter configures the reader as PTP slave only, even if no other master is active.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
mode | bool | [ON|OFF] | OFF: Disables PTP slave only configuration of the reader ON: Configures the reader as PTP slave only

## Platforms

DM80-PoE, DM280, DM290, DM360, DM370, DM390, DM470

## Notes

Version: 5.5.0