# IMAGEBUFFER.MIN-DISTANCE

Sets the minimum distance between images to buffer.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
distance | int | [1-10000] | Minimum distance in millimeters between images to buffer if IMAGEBUFFER.IMG-TYPE is 7. Default value is 150 mm.

## Platforms

DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050, DM8600.

## Notes

Version: 6.4.2 SR2