View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# QR Code Properties

Ignore Polarity

When checked, your device in trained state can read codes with polarity opposite to that of the code used for training.

Flexible Grid Size

When checked, your device in trained state can read codes with grid size slightly different (+/- one level) from that of the code used for training. That is, if you trained a 25x25 QR code, for example, with flexible grid size you will be able to decode 21x21 or 29x29 size codes, too.

Maximum Grid Size

Maximum Grid Size allows you to decode QR codes that are larger than size 49. You can either drag the slider or type in a specific code size to the text box on the right.

QR code quality metrics

For information on code quality metrics, see the DataMan Communications and Programming Guide.

Note: default, DM050, DM060, DM070, DM080, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM380, DM390, DM470, DM503, DM580