View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What data is displayed on the Trigger Performance pane?

In order for Trigger Performance to be enabled, you need to tick the Detailed Trigger Information for Good Reads option of the Data Collection list in the Settings tab.

Trigger Performance does not aggregate data for 1 minute intervals like other panes, but instead shows each trigger on the graph. Individual triggers are represented by dots on the graph and their numeric value is displayed. Plotted values (the one being monitored) can be chosen from a number of possible values in the Plotted values drop down box. Note that depending on the firmware version on the monitored device, the list of plotted values can be different.

The scrollbar can be moved to the desired point in time to view the data of that particular time. Scrollbar length can be modified (hold click and drag) to change the monitored interval. The Color plots based on setting allows you to set the criteria for the coloring of dots on the graph.

A single dot (trigger) can be clicked on the graph to display all the related data that RTM Lean collected on the right side if the trigger resulted in a good read. If it resulted in a bad read, RTM Lean displays the image taken that can be saved by clicking on the Save icon.

Note: DM060, DM080, DM260, DM280, DM290, DM300, DM360, DM370, DM380, DM390, DM470, DM503, DM580, RTM_Lean