View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do I adjust the image exposure?

Click Tune to automatically select the best settings for your reading. This initiates the Optimize Brightness and Train Code features.

NOTE: Optimize Brightness and Tune does not work if one RoI dimension is smaller than 144.

Click Optimize Brightness to automatically set a recommended light intensity. This feature is available if Manual Exposure control is selected. To enable Manual Exposure or for further settings, click the icon next to the Optimize Brightness button. Alternatively, drag the Exposure slider under the image to the left or to the right, or type in a value for the exposure. For further settings, click the icon next to the text box on the right.

You can also change the Exposure settings while experimenting with Live Display.

Note: DM050, DM060, DM070, DM080, DM150, DM260, DM280, DM290, DM360, DM370, DM380, DM390, DM470, DM503, DM580