View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is Lower-Upper if I set the Focus Steps to 1?

In Manual trigger mode only, if Focus Steps is set to 1 or 2, Focus Range is switching between the two values: a lower and an upper value. This is represented by the slider being split into two that can be changed separately.

In case of millimeter distance, the two sliders are sweep range high and sweep range low. In case of diopter, the two sliders are power range high and power range low.

Please note that the focus distance is measured from the lens, not from the front cover of the reader.

Note: DM8050, DM8070, DM8600, DM8700