View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# UPC/EAN Properties: What does the Expanded checkbox mean?

This is a Boolean to indicate whether the reported decoded string for UPC-EAN should be expanded to a 13-digit EAN13 format or transmitted in the standard UPC-E 6-digit format.

When checked (default), the decoded string is transmitted in 13 digit EAN-13 format (e.g. 0012345000065). When unchecked, the result is transmitted as <number system> + 6 data digits + <check character> (e.g. 01234565).

Note: default, DMAE50, DM050, DM060, DM070, DM080, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM380, DM390, DM470, DM503, DM580, DM7500, DM8050, DM8070, DM8600, DM8700, MX-1000, MX-1500