View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What does a blue rectangle around the barcode indicate in Symbol Diagnostics?

A blue rectangle indicates that Checksum verification of this barcode failed. Common causes for Checksum validation failure are as follows (please check the corresponding Tech Note for detailed images that illustrate each case):

- Damaged barcode (barcodes can be folded and aligned such that all the data characters decode, but it is a NoRead still, as checksum verification is not passed)

- Incorrect pattern is printed (the encoded string and the printed barcode pattern don’t match and if the symbology supports Checksum, then the decoder can indicate such failure)

Note: Note: Symbol Diagnostics is a feature that is activated exclusively by feature key.

Note: DM070, DM080, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM380, DM390, DM470, DM503, DM580