View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How can I stop Excel from skipping cells?

By default, the reader appends a carriage return/linefeed pair after each transmitted code. When you use a keyboard connection to enter the transmitted codes into Excel, the carriage return/linefeed pair causes Excel to advance by two rows after each code. To prevent this from happening, configure the reader to send only a carriage return:

1. Click on Standard Formatting.

2. Specify the symbology you are using in the Symbology tabs.

3. Check the Formatting Enabled box.

4. Click on Full string in the General tab.

5. Click Add.

6. In Terminating Text, enter \r in the text field and uncheck the CR/LF box.

Note: default, DMAE50, DM050, DM060, DM070, DM150, DM260, DM7500, DM8050, DM8070, DM8600, MX-1000, MX-1500