View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is Expanded Focus?

When Expanded Focus is enabled, the High-speed Liquid Lens steps through a defined number of planes around a central point on continuous acquisitions to attempt to read insufficiently focused codes, for example, at the limit of focus range. The default configuration allows 3 steps, but it can be set up to 10 steps.

If Expanded Focus is enabled with autofocus and the last distance input provided a distance above or below the search interval, Expanded Focus changes the central reference point for the focus step.

If no distance or height sensor is present, you can use this option to enhance the depth of field at the cost of a slower readout.

Note: DM080, DM280, DM290, DM370, DM380, DM390, DM470, DM580