View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What happens if I enable Bounded Focus Range for my Torch?

If the distance that the height sensor records is outside of the bounded focus range, it focuses to the closest boundary. Values below the minimum cause the reader to focus on the minimum and values above the maximum cause the reader to focus on the maximum. This prevents reading targets outside of the boundary range.

The default range is a minimum of 150 mm and a maximum of 1000 mm.

Please note that the focus distance is measured from the lens, not from the front cover of the reader.

Note: DM280, DM290, DM370, DM390, DM470