View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Wireless Reader Only: What is the difference between Hibernation mode and Power off?

In Hibernation mode your runtime data is saved in the memory. If you have unsaved changes to the reader, they are preserved when you pull the trigger and wake the reader up.

In Power off mode, the reader turns off and all unsaved changes are lost. By powering off the reader, you are saving energy as the battery is not in use.

In both modes you have to pull the trigger to wake the reader up.

Note: DM8050, DM8070, DM8600, DM8700